**
**
**  VIA Rhine Family Fast Ethernet Adapter
**
**  NDIS 6.20 Driver for Windows 7
**
**  v1.15   Mar, 2011
**
**

Introduction:
=============

  This document shows you how to setup the driver in Windows operating system.

Contents of the Subdirectory:
=============================

    FETN62.SYS          The NDIS 6.20 driver for Windows 7.
    NETVFX86.INF        The installation information file.
    WINX86.TXT          This file.

Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured.

    1. Turn on the power of your PC on to boot from Windows operating system.
       Windows will auto-detect your new adapter, and the "New Hardware Found"
       dialogue box will appear. Select "Driver from disk provided by hardware
       manufacturer" to install driver from the diskette that comes with your
       LAN adapter.

    2. Insert the driver diskette into your floppy drive, and specify the
       path of the driver in the diskette(i.e. A:\) to copy the driver
       files to your system.
