;
; yk62x86
; Supported hardware: Marvell Yukon Ethernet Controller
;
; (C)Copyright 2007-2012 Marvell(R).
; 
; All rights reserved.
;
; inf file for NDIS6.2 Miniport Driver for Windows 7 yk62x86.sys

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %Marvell%
CatalogFile	= yk62x86.CAT
DriverVer       = 03/23/2012, 11.45.4.3


[Manufacturer]
%Marvell%      = Marvell, NTamd64.6.1, NTx86.6.1,NTamd64.6.0, NTx86.6.0, NTamd64.5.2, NTx86.5.1

[ControlFlags]

ExcludeFromSelect       = *

;-----------------------------------------------------------------------------
;
;       Windows 2000
;
;-----------------------------------------------------------------------------
[Marvell]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows XP / Server 2003
;
;-----------------------------------------------------------------------------
[Marvell.NTx86.5.1]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows Server 2003 (64bit)
;
;-----------------------------------------------------------------------------
[Marvell.NTamd64.5.2]
;Empty section


;-----------------------------------------------------------------------------
;
;       Windows Vista
;
;-----------------------------------------------------------------------------
[Marvell.NTamd64.6.0]
;Empty section

[Marvell.NTx86.6.0]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows Windows 7
;
;-----------------------------------------------------------------------------
[Marvell.NTamd64.6.1]
;Empty section

[Marvell.NTx86.6.1]
%AT-2803.DeviceDesc% = SLYuk2CopGig_AA770E65.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_28031259
%AT-2804.DeviceDesc% = SLYuk2FibGig_35BE8B25.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_28041259
%AT-2916.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_29161259
%AT-2973_1.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_29731259
%AT-2973.DeviceDesc% = SLYukFibGig_8000C774.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_29731259
%AT-2974_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_29741259
%AT-2974.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_29741259
%AT-2978.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_29781259
%RDK-8001.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_01211148
%RDK-8002.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_02211148
%RDK-8003.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_03211148
%RDK-8004.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_04211148
%RDK-8006.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_06211148
%RDK-8007.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_07211148
%RDK-8008.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_08211148
%RDK-8009.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_09211148
%RDK-8011.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_11211148
%RDK-8012.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_12211148
%SK-9521-V2.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_32211148
%SK-9521.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_95211148
%SK-9821-V2.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50211148
%SK-9841-V2.DeviceDesc% = SLYukFibGig_311CC9CD.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50411148
%SK-9843-V2.DeviceDesc% = SLYukFibGig_311CC9CD.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50431148
%SK-9851-V2.DeviceDesc% = SLYukFibGig_311CC9CD.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50511148
%SK-9861-V2.DeviceDesc% = SLYukFibGig_311CC9CD.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50611148
%SK-9871-V2.DeviceDesc% = SLYukFibGig_311CC9CD.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50711148
%SKYukon2-2220.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_22201148
%SKYukon2-8220.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_82201148
%SKYukon2-9C21.DeviceDesc% = SLYuk2CopGig_9FA777F0.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21C01148
%SKYukon2-9E21D.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21D01148
%SKYukon2-9E21M_1.DeviceDesc% = SLYuk2CopGig_151E4536.ndi, PCI\VEN_1148&DEV_9E01&SUBSYS_21021148
%SKYukon2-9E21M.DeviceDesc% = SLYuk2CopGig_151E4536.ndi, PCI\VEN_1148&DEV_9E01&SUBSYS_21011148
%SKYukon2-9E21.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21001148
%SKYukon2-9E22.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_22001148
%SKYukon2-9E81.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_81001148
%SKYukon2-9E82.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_82001148
%SKYukon2-9E91.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_91001148
%SKYukon2-9E92.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_92001148
%SKYukon2-9I22.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_22101148
%SKYukon2-9P22.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_22101148
%SKYukon2-9P82.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_82101148
%SKYukon2-9S21.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_21001148
%SKYukon2-9S22.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_22001148
%SKYukon2-9S81.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_81001148
%SKYukon2-9S82.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_82001148
%SKYukon2-9S91.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_91001148
%SKYukon2-9S92.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_92001148
%Yukon-1032.DeviceDesc% = SLYukCopGig_65D41CE0.ndi, PCI\VEN_1737&DEV_1032&SUBSYS_00151737
%Yukon-1064.DeviceDesc% = SLYukCopGig_65D41CE0.ndi, PCI\VEN_1737&DEV_1064&SUBSYS_00161737
%Yukon-1700.DeviceDesc% = SLYukCopGig_9980B5D3.ndi, PCI\VEN_10B7&DEV_1700&SUBSYS_002010B7
%Yukon-1700_1.DeviceDesc% = SLYukCopGig_9980B5D3.ndi, PCI\VEN_10B7&DEV_1700&SUBSYS_001010B7
%Yukon-1700_1.DeviceDesc% = SLYukCopGig_9980B5D3.ndi, PCI\VEN_10B7&DEV_1700&SUBSYS_80EB1043
%Yukon-4320.DeviceDesc% = SLYukCopGig_6FBDC630.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_004715D4
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_00851025
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_00881025
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_012111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_032111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_6FBDC630.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0C19105B
%Yukon-4320.DeviceDesc% = SLYukCopGig_6FBDC630.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0CC5105B
%Yukon-4320.DeviceDesc% = SLYukCopGig_6FBDC630.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0CCF105B
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0F381019
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_102111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_6FBDC630.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1406147B
%Yukon-4320.DeviceDesc% = SLYukCopGig_2C0E4360.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_173C1043
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1C0317F2
%Yukon-4320.DeviceDesc% = SLYukCopGig_6FBDC630.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_2803270F
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_502111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_6FBDC630.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_80011019
%Yukon-4320.DeviceDesc% = SLYukCopGig_AB59B729.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_811A1043
%Yukon-4320.DeviceDesc% = SLYukCopGig_6FBDC630.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_90251695
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_952111AB
%Yukon-4320.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_E0001458
%Yukon-4340.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4340&SUBSYS_212111AB
%Yukon-4340.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_11AB&DEV_4344&SUBSYS_218111AB
%Yukon-4340.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_11AB&DEV_4344&SUBSYS_219111AB
%Yukon-4341.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_11AB&DEV_4341&SUBSYS_222211AB
%Yukon-4341.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_11AB&DEV_4345&SUBSYS_228211AB
%Yukon-4341.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_11AB&DEV_4345&SUBSYS_229211AB
%Yukon-4341.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_11AB&DEV_4341&SUBSYS_3015107B
%Yukon-4342.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4342&SUBSYS_612111AB
%Yukon-4342.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_11AB&DEV_4346&SUBSYS_618111AB
%Yukon-4342.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_11AB&DEV_4346&SUBSYS_619111AB
%Yukon-4343.DeviceDesc% = DLYuk2FibGig_8E001288.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_001A1170
%Yukon-4343.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_3015107B
%Yukon-4343.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_622211AB
%Yukon-4343.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_628211AB
%Yukon-4343.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_629211AB
%Yukon-4343.DeviceDesc% = DLYuk2CopGig_E5D307ED.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_81DA1043
%Yukon-4343.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_E0001458
%Yukon-4350.DeviceDesc% = SLYuk2CopFast_B5F98544.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_00011179
%Yukon-4350.DeviceDesc% = SLYuk2CopFast_D0BAD71A.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_00BA11AB
%Yukon-4350.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_352111AB
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_B5F98544.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00011179
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00018086
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000D1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000E1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000F1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00111854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_D0BAD71A.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001214C0
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00121854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00141854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00151854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00161854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00171854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00181854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001A1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001B1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001C1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001E1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00201854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00211854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00221854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00231854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00241854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00281854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_002A1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_002B1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_002D1854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00301854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_45EADE3F.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00311854
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_D0BAD71A.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00BA11AB
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_D0B43138.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0300107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_D0B43138.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0365107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_D0B43138.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0506107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0733152D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0748152D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_11111071
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_9984AF1D.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_203D161F
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D1B2DFA.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_3015107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D1B2DFA.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_3031107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D1B2DFA.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_3032107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_362111AB
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D1B2DFA.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_4009107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D1B2DFA.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_4038107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D1B2DFA.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_4039107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D1B2DFA.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_5052107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4D1B2DFA.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_5053107B
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_80361019
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_81E6104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_8203104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_8205104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_820F104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_8212104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_E8B7346C.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_833810F7
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_9005104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_9017104D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_902B1695
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_AC1213D1
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_2CE45675.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_C027144D
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_B5F98544.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_FF001179
%Yukon-4351.DeviceDesc% = SLYuk2CopFast_B5F98544.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_FF101179
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2A5CDBAA.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_001214C0
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2A5CDBAA.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_00241854
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2A5CDBAA.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_00BA11AB
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2A5CDBAA.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_01011025
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_CAFE449C.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_01101025
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2047CAE0.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0317107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2047CAE0.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0318107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2A5CDBAA.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0366107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2047CAE0.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0367107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2047CAE0.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0507107B
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2047CAE0.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_06201558
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2047CAE0.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0753152D
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2047CAE0.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_0754152D
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_1C0317F2
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_D8A0578B.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_2054161F
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_684AB0D9.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_666617AA
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_80381019
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_902D1695
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_E9001631
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_2A5CDBAA.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_F50117FF
%Yukon-4352.DeviceDesc% = SLYuk2CopFast_04E0C659.ndi, PCI\VEN_11AB&DEV_4352&SUBSYS_FF101179
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_D0BAD71A.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_00BA11AB
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01041854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01051854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01061854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01071854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01081854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01091854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_010E1854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_010F1854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_011B1854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_011C1854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_011D1854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_011E1854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_011F1854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01201854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01211854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01221854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01231854
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_01241025
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_022E1028
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_022F1028
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_05025FBF.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_023A1028
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_9D8DA62E.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_0366107B
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_9D8DA62E.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_0367107B
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_DCA95EB8.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_059317FF
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_DCA95EB8.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_0761152D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_DCA95EB8.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_0769152D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_0CE7105B
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_D0BAD71A.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_26711019
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_DCA95EB8.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_2E301509
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_DCA95EB8.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_2F021509
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_170ACBC1.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_303017AA
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_170ACBC1.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_303617AA
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_170ACBC1.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_303A17AA
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_CB09DB20.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_30CD103C
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_6B2708F9.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_30E4103C
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_6B2708F9.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_30E8103C
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_6B2708F9.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_30E9103C
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_1083B51F.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_666617AA
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_80391019
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_9005104D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_9017104D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_4EF04A88.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_902D104D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_877C7536.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_B048144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_877C7536.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_B04B144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_2CE45675.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C031144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_2CE45675.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C034144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_2CE45675.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C038144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_2CE45675.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C03C144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C1021631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C1031631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C1041631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C1051631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C20B1631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C20D1631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_61633276.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C20E1631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_2CE45675.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C510144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_2CE45675.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_C517144D
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_0F3A0130.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_E9001631
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_B5F98544.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_FF101179
%Yukon-4353.DeviceDesc% = SLYuk2CopFast_B5F98544.ndi, PCI\VEN_11AB&DEV_4353&SUBSYS_FF131179
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_AED03A1E.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_00BA11AB
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_2E58636B.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_01241025
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_3D4C8180.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_01361854
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_3D4C8180.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_01371854
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E2B78E5F.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0185107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_D29BE4FD.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_022E1028
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_D29BE4FD.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_022F1028
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_D29BE4FD.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_023A1028
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E2B78E5F.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_028E1028
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E2B78E5F.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_02AA1028
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0390107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0391107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0395107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0396107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E2B78E5F.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_04061028
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0580107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0581107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0585107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0586107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0590107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0591107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0595107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0596107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0700107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0701107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0800107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_89B90F86.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0801107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_45CF430A.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_0CDB105B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E2B78E5F.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_1085107B
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_C5A328B2.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_144C10CF
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E2B78E5F.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_2AAA1028
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_2E58636B.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_30041509
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E9362899.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_305417AA
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_B069D0AD.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_307D103C
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E2B78E5F.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_361A103C
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E2B78E5F.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_4300103C
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_72D5C317.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_63011682
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_72D5C317.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_71501AFA
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_D7DDA87B.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_80401AFA
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_F35B0AEC.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_9033104D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_F35B0AEC.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_903F104D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_F35B0AEC.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_9044104D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_CC92B7F9.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B048144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_CC92B7F9.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B04B144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_02C24B51.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B051144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_CC92B7F9.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B058144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B061144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B062144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B063144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B064144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B065144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_B066144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C02F144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C031144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C033144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C034144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C038144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C03B144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C03C144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_AA300557.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C03D144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C03E144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C03F144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E490EEE0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C040144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E490EEE0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C041144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_BF875FF5.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C042144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C043144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E490EEE0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C046144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C047144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C048144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C049144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C04A144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C04B144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C04D144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_7E3EB2A6.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C04E144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C04F144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C050144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C051144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C052144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C053144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C054144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C055144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C057144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C058144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C059144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C05A144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C05B144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C05C144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C05D144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C05E144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C05F144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C060144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C061144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C062144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C509144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C510144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C517144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E490EEE0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C518144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E490EEE0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C519144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_E490EEE0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C520144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C521144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C540144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C541144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C542144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C543144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C544144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C545144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C546144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C547144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C548144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_C549144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_BF875FF5.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_CA00144D
%Yukon-4354.DeviceDesc% = SLYuk2CopFast_EA568FF0.ndi, PCI\VEN_11AB&DEV_4354&SUBSYS_CA01144D
%Yukon-4355.DeviceDesc% = SLYuk2CopFast_95C9A6C2.ndi, PCI\VEN_11AB&DEV_4355&SUBSYS_111311AB
%Yukon-4355.DeviceDesc% = SLYuk2CopFast_A3DC0B36.ndi, PCI\VEN_11AB&DEV_4355&SUBSYS_FF501179
%Yukon-4356.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4356&SUBSYS_2A35103C
%Yukon-4356.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4356&SUBSYS_2A36103C
%Yukon-4356.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4356&SUBSYS_2A37103C
%Yukon-4356.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4356&SUBSYS_2A46103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_55BABACC.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_00BA11AB
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_47BFE533.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_02531028
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_516409D5.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_308A103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_516409D5.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_308B103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_516409D5.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_308C103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_516409D5.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_308D103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_8C4CCC12.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_30E4103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_8C4CCC12.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_30E8103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_8C4CCC12.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_30E9103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_2944A77E.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_30F3103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_2944A77E.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_30F7103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_2944A77E.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_30FB103C
%Yukon-4357.DeviceDesc% = SLYuk2CopFast_2944A77E.ndi, PCI\VEN_11AB&DEV_4357&SUBSYS_30FC103C
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_00861025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_00871025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_008D1025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_008E1025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_3FAD912D.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_01231025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_3FAD912D.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_01241025
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_E4941365.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0300107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_E4941365.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0506107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0509A0A0
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_052C1462
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0C36105B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_110115BD
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3015107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3031107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3032107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4009107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4038107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4039107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_5052107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_5053107B
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_522111AB
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_80521849
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_B057CDDE.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_81341043
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_E0001458
%Yukon-4360.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_E0001940
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_E4941365.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_0300107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_E4941365.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_0506107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_3015107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_3031107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_3032107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_30638086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34398086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343A8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343B8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343C8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343D8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343E8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34508086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34518086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34528086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34538086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34588086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34598086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345A8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345B8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345C8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345D8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345E8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345F8086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34608086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34618086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34628086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34638086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34648086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34658086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34668086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34678086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_4009107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_4038107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_4039107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_502111AB
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_50218086
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_5052107B
%Yukon-4361.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_5053107B
%Yukon-4362.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00461737
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_F55D7ABE.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00011179
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000217C0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00031290
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000B1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000C1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00101854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_C3EA2072.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001214C0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00131854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00191854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001D1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001F1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00241854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00291854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_002C1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_002F1854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_71CAFC62.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00321854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00BA11AB
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_01111071
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E4941365.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0300107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_038A1558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_04A01558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E4941365.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0506107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0506A0A0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05601558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05701558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_058517FF
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_058C1462
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05901558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05911558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05921558
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_061DA0A0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_061EA0A0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0733152D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0748152D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0CA9105B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0CAA105B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0CAB105B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0CAC105B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_100315BD
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_10B717C0
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_110215BD
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_944E22C0.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_11D51043
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_2F1A3AFB.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_203C161F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_2F1A3AFB.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_203D161F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_2F1A3AFB.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_204A161F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_204E161F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2801270F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2A0D103C
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2C0817F2
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3015107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3031107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3032107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3197109F
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_4009107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_4038107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_4039107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_5052107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18667905.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_5053107B
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_532111AB
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_61001584
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_62501462
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80011854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80031854
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80531019
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80531849
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D35014FA.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80531AFA
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_B057CDDE.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81421043
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81E6104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81E8104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81E9104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81FE104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_8205104D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_5E29A18A.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_833810F7
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_90291695
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_A43010FD
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_AC1113D1
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_FF97B08B.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_B039144D
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2401297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2411297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2421297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2431297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2441297
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_E0001458
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_E0001940
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_F55D7ABE.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_FF001179
%Yukon-4362_1.DeviceDesc% = SLYuk2CopGig_F55D7ABE.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_FF101179
%Yukon-4362_2.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_AB1214EA
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_00241854
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_6A37CB5E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_002814C0
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_006C1025
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_B0A80FCE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_00791854
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_B0A80FCE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_007A1854
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_00BA11AB
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_EA9D8E20.ndi, PCI\VEN_11AB&DEV_436D&SUBSYS_00BA11AB
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_3D4429EC.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_01101025
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_C97E2004.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_02531028
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0317107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0318107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0507107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_05711558
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_06BEEAAE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0580107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_06BEEAAE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0581107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_06BEEAAE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0585107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_06BEEAAE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0586107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_06BEEAAE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0590107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_059017FF
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_06BEEAAE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0591107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_059217FF
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_06BEEAAE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0595107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_06BEEAAE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0596107B
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0753152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0754152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0761152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0762152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_0763152D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_C0734E10.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_10BE17C0
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_65F8DE1E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_10C11734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_65F8DE1E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_10D71734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_9490202C.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_110F1734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_9490202C.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_11101734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_9490202C.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_11171734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_9490202C.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_11181734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_9490202C.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_111F1734
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_509D75E0.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_11D51043
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_9363CB6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_139A10CF
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_40A984AC.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_14A910CF
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_118586BB.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_14AB10CF
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_C97E2004.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_17051043
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_65F8DE1E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_202317C0
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_2F1A3AFB.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_2054161F
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_2C201059
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_9AE47B80.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_2F121059
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_AD1F4DCD.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_2F161509
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_AD1F4DCD.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_2F171509
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_AD1F4DCD.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_30051509
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_6C64F8FD.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_30D4103C
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_29E3A05B.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_4363144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_61001584
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_7E8969BB.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_666617AA
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_81E6104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_81FE104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_8208104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_BFECC077.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_820B104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_8210104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_2753764C.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_833810F7
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_6A37CB5E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_88751033
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9008104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_900E104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_BFECC077.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_900F104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9014104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9016104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9018104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9026104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_902F1695
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_A1824401.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9034104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_3BCC2189.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9035104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_903B104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_903C104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_903D104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_3BCC2189.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9040104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_3BCC2189.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9045104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F86EDF6E.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_9048104D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_70185369.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_B051144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_5DC89192.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_B058144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C02F144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C031144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C033144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C034144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C03B144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C03E144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C03F144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C041144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C042144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C043144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_2CA29F76.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C048144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_2CA29F76.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C04A144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_91882F2A.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C04D144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C1031631
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C1041631
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C1051631
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_D7FDA790.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C20B1631
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C509144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C518144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C519144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C520144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_57BC1D95.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_C521144D
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F55D7ABE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_FF101179
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_F55D7ABE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_FF131179
%Yukon-4363.DeviceDesc% = SLYuk2CopGig_6F04C6FE.ndi, PCI\VEN_11AB&DEV_4363&SUBSYS_FF501179
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_B057CDDE.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_01501025
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C75105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7A1053
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7A105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7B105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7C105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7D105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0C7E105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0CBF105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0CCA105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0CE7105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0D10105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0D49105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0DF9105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0E09105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_0E0A105B
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_65C2B7F6.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_101F17AA
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_B057CDDE.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_14951043
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_1C0417F2
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_E4AB22B7.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_27001565
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_300319DB
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_C46AD737.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_303A17AA
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_C46AD737.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_303B17AA
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_C46AD737.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_304417AA
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_326C1462
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_B057CDDE.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_357C1462
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_562111AB
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_80CA4F7E.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_63011682
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_80CA4F7E.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_71501AFA
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_73261462
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_B057CDDE.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_80401462
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_80561019
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_D35014FA.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_80561AFA
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_B057CDDE.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_81F81043
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_E3CD965A.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_826E1043
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_B057CDDE.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_82791043
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_90321695
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_D6028086
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_E0001458
%Yukon-4364.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4364&SUBSYS_E9001631
%Yukon-4365.DeviceDesc% = SLYuk2CopGig_8833731D.ndi, PCI\VEN_11AB&DEV_4365&SUBSYS_00BA11AB
%Yukon-4365.DeviceDesc% = SLYuk2CopGig_7136A9E5.ndi, PCI\VEN_11AB&DEV_4365&SUBSYS_0E15105B
%Yukon-4365.DeviceDesc% = SLYuk2CopGig_DC92093C.ndi, PCI\VEN_11AB&DEV_4365&SUBSYS_170010B7
%Yukon-4365.DeviceDesc% = SLYuk2CopGig_239614EA.ndi, PCI\VEN_11AB&DEV_4365&SUBSYS_303F17AA
%Yukon-4365.DeviceDesc% = SLYuk2CopGig_239614EA.ndi, PCI\VEN_11AB&DEV_4365&SUBSYS_304017AA
%Yukon-4365.DeviceDesc% = SLYuk2CopGig_239614EA.ndi, PCI\VEN_11AB&DEV_4365&SUBSYS_304517AA
%Yukon-4365.DeviceDesc% = SLYuk2CopGig_239614EA.ndi, PCI\VEN_11AB&DEV_4365&SUBSYS_305817AA
%Yukon-4366.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4366&SUBSYS_2A35103C
%Yukon-4366.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4366&SUBSYS_2A36103C
%Yukon-4369.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4369&SUBSYS_00BA11AB
%Yukon-4369.DeviceDesc% = SLYuk2CopGig_3B1A236D.ndi, PCI\VEN_11AB&DEV_4369&SUBSYS_80561019
%Yukon-436A.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_436A&SUBSYS_00BA11AB
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_E39BBD9D.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_0001103C
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_B0CAB161.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_002814c0
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_8833731D.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_00BA11AB
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_AC6FE6B9.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01231025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_AC6FE6B9.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01241025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_44A6BF92.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_013F1025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_014E1025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_014F1025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01551025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01631025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01641025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_19B0635B.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01831025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_DC3704DC.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01881631
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01901025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_01911025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_BDD944D1.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_023C1025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_024E1025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_024F1025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_B0CAB161.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_02531028
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_C454C75C.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_02571025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_025B1025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_02681025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_ADB34104.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_02E81025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_031F1025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_19B0635B.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_04261025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_19B0635B.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_05901025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_DC3704DC.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_0696107B
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_7136A9E5.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_0E08105B
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_7136A9E5.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_0E12105B
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_7136A9E5.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_0E15105B
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_AC6FE6B9.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_10C417C0
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_239614EA.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_303017AA
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_239614EA.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_303617AA
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_239614EA.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_303A17AA
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_582CABC1.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_306517AA
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_99213944.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_63011682
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_3BF1F78E.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_76071025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_19B0635B.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_80001025
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_90011631
%Yukon-436B.DeviceDesc% = SLYuk2CopGig_BA1D7449.ndi, PCI\VEN_11AB&DEV_436B&SUBSYS_ACBA11AB
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_B0CAB161.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_002814C0
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_9F3A77B1.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_00BA11AB
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_B0CAB161.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_02531028
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_E00594FB.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_0700107B
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_E00594FB.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_0701107B
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_E00594FB.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_0704107B
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_E00594FB.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_0705107B
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_E00594FB.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_0750107B
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_19BDE0FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_111111AB
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_BAC35220.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_111211AB
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_3785B560.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_111311AB
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_53A53D52.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_11D51043
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_1722103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_1723103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_1724103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_1725103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_1726103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_1727103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_1728103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_1729103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_8B3E3C01.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3037103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3056103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3072103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3073103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3074103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3075103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3076103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3077103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3078103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3079103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_307A103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_307E103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_307F103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3080103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3081103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_ACC7D6F4.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_30D4103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_ACC7D6F4.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_30E4103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_ACC7D6F4.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_30E8103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_ACC7D6F4.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_30E9103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_D0298D14.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_30F4103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_D0298D14.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_30F8103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3632103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3634103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3653103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_3655103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_7011103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_7013103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_7015103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_7016103C
%Yukon-436C.DeviceDesc% = SLYuk2CopGig_56C902EE.ndi, PCI\VEN_11AB&DEV_436C&SUBSYS_FF501179
%Yukon-4370.DeviceDesc% = SLYuk2CopGig_8833731D.ndi, PCI\VEN_11AB&DEV_4370&SUBSYS_00BA11AB
%Yukon-4370.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_4370&SUBSYS_014F1025
%Yukon-4370.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_4370&SUBSYS_01621025
%Yukon-4370.DeviceDesc% = SLYuk2CopGig_D43EC289.ndi, PCI\VEN_11AB&DEV_4370&SUBSYS_025B1025
%Yukon-4370.DeviceDesc% = SLYuk2CopGig_7136A9E5.ndi, PCI\VEN_11AB&DEV_4370&SUBSYS_0E08105B
%Yukon-4370.DeviceDesc% = SLYuk2CopGig_7136A9E5.ndi, PCI\VEN_11AB&DEV_4370&SUBSYS_0E12105B
%Yukon-4370.DeviceDesc% = SLYuk2CopGig_239614EA.ndi, PCI\VEN_11AB&DEV_4370&SUBSYS_304517AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_D963382A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_00BA11AB
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_A96D667B.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_01881631
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_DC3704DC.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_02E81025
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0390107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0391107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0395107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0396107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_A96D667B.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0696107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0C650D17.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0700107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0701107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0C650D17.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0704107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0705107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0750107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0800107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_AB8461FA.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_0801107B
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_FCA57897.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_107C17C0
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_FCA57897.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_10C717C0
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_E36451B4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_110315BD
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_B0A0F888.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_14AA10CF
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_9C93F41B.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_14AC10CF
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_9C93F41B.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_14EB10CF
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_301B17AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_301C17AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_304F17AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_305217AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_305817AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_305C17AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_305D17AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_305E17AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_305F17AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_0A175BB4.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_306617AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_8AF1FD94.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_309317AA
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_FDFC7F9F.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_31651297
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_1F84F5EB.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_6C0B1057
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_1F84F5EB.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_6C0C1057
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_23259509.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_6C0E1057
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_9039104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_9040104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_9056104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_905E104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_905F104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_9063104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_9067104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_906B104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_9071104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_85C2AB2A.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_9072104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_4D658302.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_9079104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_4D658302.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_907A104D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_3E57BF88.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_B051144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_F949E04B.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_B058144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_2F0926CE.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_B061144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_B062144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_B063144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_B064144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_B065144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_B066144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C02F144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C031144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C033144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C03B144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C03E144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C03F144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C041144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C042144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C043144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_2F0926CE.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C047144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C048144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_2F0926CE.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C049144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C04A144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_2F0926CE.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C04B144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C04D144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_2F0926CE.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C04F144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_2F0926CE.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C050144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C051144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C053144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C054144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C055144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C056144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C057144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C058144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C059144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C05A144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C05B144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C05C144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C05D144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C05E144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C05F144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C060144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C061144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C062144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C509144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C519144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C520144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C521144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C540144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C541144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C542144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C543144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C544144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C545144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C546144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C547144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C548144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_90AE6613.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_C549144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_2F0926CE.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_CA00144D
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_A05E023B.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_CDCD11AB
%Yukon-4380.DeviceDesc% = SLYuk2CopGig_D471A396.ndi, PCI\VEN_11AB&DEV_4380&SUBSYS_FEFE11AB
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_151E4536.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_00BA11AB
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_7136A9E5.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_00BD1014
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_0A39381F.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_111311AB
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_1455103C
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_1608103C
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_3D7A1068.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_2B20103C
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_3D7A1068.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_2B21103C
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_32C1E8FC.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_3653103C
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_3D7A1068.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_80001025
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_18D12FBD.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_84391043
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_A7E6EE8A.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_9067104D
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_A7E6EE8A.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_9069104D
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_A7E6EE8A.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_906A104D
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_80C71EAF.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_9071104D
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_A7E6EE8A.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_9072104D
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_A7E6EE8A.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_9073104D
%Yukon-4381.DeviceDesc% = SLYuk2CopGig_80C71EAF.ndi, PCI\VEN_11AB&DEV_4381&SUBSYS_9074104D
%Yukon-4382.DeviceDesc% = SLYuk2CopGig_396F1EAE.ndi, PCI\VEN_11AB&DEV_4382&SUBSYS_00BA11AB
%Yukon-4382.DeviceDesc% = SLYuk2CopGig_B2DA9517.ndi, PCI\VEN_11AB&DEV_4382&SUBSYS_EDAC11AB
%Yukon-Generic_10.DeviceDesc% = SLYuk2CopFast_55BABACC.ndi, PCI\VEN_11AB&DEV_435A
%Yukon-Generic_11.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4361
%Yukon-Generic_12.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4360
%Yukon-Generic_13.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4362
%Yukon-Generic_14.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4363
%Yukon-Generic_14.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_436D
%Yukon-Generic_15.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4364
%Yukon-Generic_16.DeviceDesc% = SLYuk2CopGig_A05E023B.ndi, PCI\VEN_11AB&DEV_4380
%Yukon-Generic_17.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_436A
%Yukon-Generic_18.DeviceDesc% = SLYuk2CopGig_38CB86BF.ndi, PCI\VEN_11AB&DEV_4381
%Yukon-Generic_19.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4342
%Yukon-Generic_19.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_11AB&DEV_4346
%Yukon-Generic_1.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4340
%Yukon-Generic_1.DeviceDesc% = SLYuk2FibGig_B0382D73.ndi, PCI\VEN_11AB&DEV_4344
%Yukon-Generic_20.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_11AB&DEV_4343
%Yukon-Generic_20.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_11AB&DEV_4347
%Yukon-Generic_21.DeviceDesc% = SLYuk2CopGig_EB4C8BA8.ndi, PCI\VEN_11AB&DEV_4365
%Yukon-Generic_22.DeviceDesc% = SLYuk2CopGig_EB4C8BA8.ndi, PCI\VEN_11AB&DEV_436B
%Yukon-Generic_23.DeviceDesc% = SLYuk2CopGig_A0B7A9C4.ndi, PCI\VEN_11AB&DEV_436C
%Yukon-Generic_24.DeviceDesc% = SLYuk2CopGig_EB4C8BA8.ndi, PCI\VEN_11AB&DEV_4370
%Yukon-Generic_25.DeviceDesc% = SLYuk2CopGig_149A5B06.ndi, PCI\VEN_11AB&DEV_4382
%Yukon-Generic_26.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4367
%Yukon-Generic_27.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4356
%Yukon-Generic_28.DeviceDesc% = SLYuk2CopGig_E49AF547.ndi, PCI\VEN_11AB&DEV_4368
%Yukon-Generic_29.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4366
%Yukon-Generic_2.DeviceDesc% = DLYuk2CopGig_08C066A8.ndi, PCI\VEN_11AB&DEV_4341
%Yukon-Generic_2.DeviceDesc% = DLYuk2FibGig_B503A37E.ndi, PCI\VEN_11AB&DEV_4345
%Yukon-Generic_30.DeviceDesc% = SLYuk2CopGig_18689F27.ndi, PCI\VEN_11AB&DEV_4369
%Yukon-Generic_3.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4350
%Yukon-Generic_4.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4351
%Yukon-Generic_5.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4352
%Yukon-Generic_6.DeviceDesc% = SLYuk2CopFast_4D15CBD8.ndi, PCI\VEN_11AB&DEV_4353
%Yukon-Generic_7.DeviceDesc% = SLYuk2CopFast_FDC7536D.ndi, PCI\VEN_11AB&DEV_4354
%Yukon-Generic_8.DeviceDesc% = SLYuk2CopFast_55BABACC.ndi, PCI\VEN_11AB&DEV_4355
%Yukon-Generic_9.DeviceDesc% = SLYuk2CopFast_55BABACC.ndi, PCI\VEN_11AB&DEV_4357
%Yukon-Generic.DeviceDesc% = SLYukCopGig_2BA069C3.ndi, PCI\VEN_11AB&DEV_4320


;-------------------------------------------------------------------------------
; 

[DLYuk2CopGig_08C066A8.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WoLAll

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_DL, yk62x86.GigFrSize.params, yk62x86.DLSpeedDuplexGig.params, yk62x86.DualLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[DLYuk2CopGig_08C066A8.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[DLYuk2CopGig_E5D307ED.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WoLAll

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_DL, yk62x86.GigFrSize.params, yk62x86.DLSpeedDuplexGig.params, yk62x86.DualLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.EnergyStarON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[DLYuk2CopGig_E5D307ED.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[DLYuk2FibGig_8E001288.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_DL, yk62x86.GigFrSize.params, yk62x86.DualLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[DLYuk2FibGig_8E001288.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 
[SLYuk2FibGig_35BE8B25.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2FibGig_35BE8B25.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 
 
[DLYuk2FibGig_B503A37E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_DL, yk62x86.GigFrSize.params, yk62x86.DualLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[DLYuk2FibGig_B503A37E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_02C24B51.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_02C24B51.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_04E0C659.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.TcpLargeSend

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegmLSOff.params, yk62x86.TxRxLE.params, yk62x86.BatMaxRed.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_04E0C659.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_05025FBF.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_05025FBF.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_0F3A0130.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_0F3A0130.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_1083B51F.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMaxRed.params, yk62x86.WfSON.params, yk62x86.WoLMagicPkt.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_1083B51F.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_170ACBC1.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSON.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_170ACBC1.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_2047CAE0.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMaxRed.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_2047CAE0.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_2944A77E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_2944A77E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_2A5CDBAA.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMaxRed.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_2A5CDBAA.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_2CE45675.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSOFF.params, yk62x86.FullBatDefaults.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_2CE45675.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_2E58636B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_2E58636B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_3D4C8180.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.PropPage_PMChkBox_xx0.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_3D4C8180.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_45CF430A.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_45CF430A.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_45EADE3F.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_45EADE3F.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_47BFE533.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_47BFE533.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_4D15CBD8.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_4D15CBD8.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_4D1B2DFA.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLMagicPkt.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_4D1B2DFA.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_4EF04A88.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_4EF04A88.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_516409D5.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_516409D5.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_55BABACC.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_55BABACC.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_61633276.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_61633276.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_684AB0D9.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMaxRed.params, yk62x86.WfSON.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_684AB0D9.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_6B2708F9.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_6B2708F9.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_72D5C317.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_72D5C317.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_7E3EB2A6.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WfSOFF.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.MonitorSpeedStep.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_7E3EB2A6.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_877C7536.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSON.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_877C7536.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_89B90F86.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPkt.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_89B90F86.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_8C4CCC12.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_8C4CCC12.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_95C9A6C2.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange
DelReg          = yk62x86.delreg.TcpLargeSend
DelReg          = yk62x86.delreg.PatternMatch
DelReg          = yk62x86.delreg.MagPackPattMatch

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegmLSOff.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPacketDefault.params, yk62x86.WoLMagicPktOnly.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_2.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_95C9A6C2.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_9984AF1D.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_9984AF1D.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_9D8DA62E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMaxRed.params, yk62x86.WoLNoLnkCh.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_9D8DA62E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_A3DC0B36.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange
DelReg          = yk62x86.delreg.TcpLargeSend

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegmLSOff.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPacketDefault.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_2.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_A3DC0B36.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_AA300557.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WfSON.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_AA300557.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_AED03A1E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_AED03A1E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_B069D0AD.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam
DelReg          = yk62x86.delreg.SmartPowMgmt

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSON.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_B069D0AD.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_B5F98544.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange
DelReg          = yk62x86.delreg.TcpLargeSend

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegmLSOff.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPkt.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_B5F98544.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_BF875FF5.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WfSOFF.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_BF875FF5.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_C5A328B2.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_C5A328B2.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_CAFE449C.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMaxRed.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_CAFE449C.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_CB09DB20.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSON.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_CB09DB20.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_CC92B7F9.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_CC92B7F9.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_D0B43138.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPkt.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_D0B43138.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_D0BAD71A.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_D0BAD71A.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_D29BE4FD.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_D29BE4FD.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_D7DDA87B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_D7DDA87B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_D8A0578B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMaxRed.params, yk62x86.WoLNoLnkCh.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_D8A0578B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_DCA95EB8.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_DCA95EB8.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_E2B78E5F.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_E2B78E5F.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_E490EEE0.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WfSOFF.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_E490EEE0.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_E8B7346C.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_E8B7346C.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_E9362899.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSOFF.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_4.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_E9362899.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_EA568FF0.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_EA568FF0.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_F35B0AEC.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_F35B0AEC.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopFast_FDC7536D.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplex.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopFast_FDC7536D.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_06BEEAAE.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPkt.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_06BEEAAE.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_0A175BB4.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSOFF.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_8.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_0A175BB4.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_0A39381F.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmartDeep.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_0A39381F.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_0C650D17.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_0C650D17.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_118586BB.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.EnergyStarON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_118586BB.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_149A5B06.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_149A5B06.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_151E4536.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_151E4536.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_18667905.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLMagicPkt.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_18667905.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_18689F27.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_18689F27.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_18D12FBD.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_18D12FBD.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_19B0635B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLMagicPkt.params, yk62x86.PropPage_PMChkBox_xxx.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_19B0635B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_19BDE0FC.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.SmartPowMgmt

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_11.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_19BDE0FC.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_1F84F5EB.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_7.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_1F84F5EB.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_23259509.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_23259509.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_239614EA.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSOFF.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_4.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_239614EA.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_2753764C.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.JumboPacket

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.FastFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_2753764C.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_29E3A05B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_29E3A05B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_2CA29F76.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WfSOFF.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_2CA29F76.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_2F0926CE.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WfSOFF.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_2F0926CE.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_2F1A3AFB.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_2F1A3AFB.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_32C1E8FC.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam
DelReg          = yk62x86.delreg.SmartPowMgmt

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_32C1E8FC.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_3785B560.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange
DelReg          = yk62x86.delreg.PatternMatch
DelReg          = yk62x86.delreg.MagPackPattMatch

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegmLSOff.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPacketDefault.params, yk62x86.WoLMagicPktOnly.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_2.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_3785B560.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_38CB86BF.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_38CB86BF.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_396F1EAE.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_396F1EAE.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_3B1A236D.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_3B1A236D.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_3BCC2189.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_5.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_3BCC2189.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_3BF1F78E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_3BF1F78E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_3D4429EC.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_3D4429EC.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_3D7A1068.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLW10.params, yk62x86.WoLMagicPkt.params, yk62x86.PropPage_PMChkBox_xxx.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_3D7A1068.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_3E57BF88.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_3E57BF88.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_3FAD912D.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_3FAD912D.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_40A984AC.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.EnergyStarON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_40A984AC.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_44A6BF92.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_44A6BF92.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_4D658302.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.PropPage_PMChkBox_x00.params, yk62x86.DefaultWfSOFF.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_4D658302.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_509D75E0.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_509D75E0.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_53A53D52.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_53A53D52.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_56C902EE.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange
DelReg          = yk62x86.delreg.TcpLargeSend

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegmLSOff.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPacketDefault.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_2.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_56C902EE.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_57BC1D95.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WfSOFF.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_57BC1D95.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_582CABC1.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLMagicPkt.params, yk62x86.EnergyStarON.params, yk62x86.PropPage_PMChkBox_xxx.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_4.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_582CABC1.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_5DC89192.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_5DC89192.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_5E29A18A.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_5E29A18A.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_65C2B7F6.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSON.params, yk62x86.WoLNoLnkCh.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_65C2B7F6.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_65F8DE1E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLWfSForcedCombine.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_65F8DE1E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_6A37CB5E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_6A37CB5E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_6C64F8FD.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_6C64F8FD.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_6F04C6FE.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange
DelReg          = yk62x86.delreg.TcpLargeSend

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegmLSOff.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_6F04C6FE.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_70185369.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSOFF.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_70185369.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_7136A9E5.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_7136A9E5.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_71CAFC62.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_71CAFC62.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_7E8969BB.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSON.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_7E8969BB.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_80C71EAF.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.PropPage_PMChkBox_x00.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_80C71EAF.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_80CA4F7E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_80CA4F7E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_85C2AB2A.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_85C2AB2A.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_8833731D.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_8833731D.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_8AF1FD94.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSOFF.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_9.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_8AF1FD94.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_8B3E3C01.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_8B3E3C01.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_90AE6613.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_90AE6613.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_91882F2A.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WfSOFF.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.MonitorSpeedStep.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_91882F2A.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_9363CB6E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLWfSForcedCombine.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_9363CB6E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_944E22C0.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_944E22C0.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_9490202C.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.EnergyStarON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_9490202C.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_99213944.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_99213944.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_9AE47B80.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_9AE47B80.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_9C93F41B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL
DelReg          = yk62x86.delreg.MaxPwrSaveMode
DelReg          = yk62x86.delreg.SmartPowMgmt

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.EnergyStarON.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_9C93F41B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_9F3A77B1.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_9F3A77B1.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_9FA777F0.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_9FA777F0.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_A05E023B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_A05E023B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_A0B7A9C4.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_A0B7A9C4.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_A1824401.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_A1824401.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_A7E6EE8A.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_A7E6EE8A.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_A96D667B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_A96D667B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_AB8461FA.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLMagicPkt.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_AB8461FA.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_AC6FE6B9.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_AC6FE6B9.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_ACC7D6F4.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_ACC7D6F4.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_AD1F4DCD.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_AD1F4DCD.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_ADB34104.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_ADB34104.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_B057CDDE.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_B057CDDE.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_B0A0F888.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLWfSForcedCombine.params, yk62x86.EnergyStarON.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_B0A0F888.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_B0A80FCE.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSON.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_B0A80FCE.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_B0CAB161.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_B0CAB161.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_B2DA9517.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_B2DA9517.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_BA1D7449.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.SmartPowMgmt.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_BA1D7449.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_BAC35220.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam
DelReg          = yk62x86.delreg.SmartPowMgmt

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSOFF.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_11.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_BAC35220.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_BDD944D1.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_BDD944D1.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_BFECC077.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.SmartBatDefaults.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_BFECC077.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_C0734E10.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSL

AddReg          = yk62x86.reg, yk62x86.commonMsgLogOff.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLWfSForcedCombine.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_C0734E10.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_C3EA2072.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_C3EA2072.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_C454C75C.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_C454C75C.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_C46AD737.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSOFF.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_4.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_C46AD737.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_C97E2004.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_C97E2004.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_D0298D14.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.WfSSLParam

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WfSS5MagicPacket.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_D0298D14.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_D35014FA.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_D35014FA.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_D43EC289.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_D43EC289.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_D471A396.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmartDeep.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params, yk62x86.MonitorSpeedStep.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_D471A396.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_D7FDA790.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_D7FDA790.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_D963382A.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_D963382A.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_DC3704DC.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_DC3704DC.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_DC92093C.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.MaxPwrSaveMode

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_10.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_DC92093C.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_E00594FB.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPkt.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_E00594FB.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_E36451B4.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarOFF.params, yk62x86.DefaultWfSOFF.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_E36451B4.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_E39BBD9D.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.BatMaxDefaults.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_3.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_E39BBD9D.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_E3CD965A.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_E3CD965A.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_E4941365.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPkt.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_E4941365.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_E49AF547.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_E49AF547.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_E4AB22B7.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLinkFCOff.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_E4AB22B7.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_EA9D8E20.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_6.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_EA9D8E20.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_EB4C8BA8.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_EB4C8BA8.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_F55D7ABE.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.LinkChange
DelReg          = yk62x86.delreg.TcpLargeSend

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegmLSOff.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLMagicPkt.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_F55D7ABE.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_AA770E65.ndi.NTx86]
DelReg          = yk62x86.delreg.Common
DelReg          = yk62x86.delreg.BatParams
DelReg          = yk62x86.delreg.SpeedDuplexNot100

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplex_100M_only.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.IPv6.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_AA770E65.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_F86EDF6E.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLW10.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_F86EDF6E.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_F949E04B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatSmart.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_F949E04B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_FCA57897.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.BatMax.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_FCA57897.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_FDFC7F9F.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WoLNoLnkCh.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params, yk62x86.HwFeaDev_1.params, yk62x86.RSS.params, yk62x86.LSoV2.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_FDFC7F9F.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2CopGig_FF97B08B.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params, yk62x86.WfSON.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2CopGig_FF97B08B.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYuk2FibGig_B0382D73.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SingleLink.params, yk62x86.TCPSegm.params, yk62x86.TxRxLE.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYuk2FibGig_B0382D73.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYukCopGig_2BA069C3.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TxRxBuff.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYukCopGig_2BA069C3.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYukCopGig_2C0E4360.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TxRxBuff.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYukCopGig_2C0E4360.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYukCopGig_65D41CE0.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TxRxBuff.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYukCopGig_65D41CE0.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYukCopGig_6FBDC630.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TxRxBuff.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYukCopGig_6FBDC630.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYukCopGig_9980B5D3.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TxRxBuff.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSON.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYukCopGig_9980B5D3.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYukCopGig_AB59B729.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SLSpeedDuplexGig.params, yk62x86.SingleLink.params, yk62x86.TxRxBuff.params, yk62x86.WoLStd.params, yk62x86.EnergyStarON.params, yk62x86.DefaultWfSOFF.params, yk62x86.HwFeaDev_1.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYukCopGig_AB59B729.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYukFibGig_311CC9CD.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SingleLink.params, yk62x86.TxRxBuff.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYukFibGig_311CC9CD.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog

;-------------------------------------------------------------------------------
; 

[SLYukFibGig_8000C774.ndi.NTx86]
DelReg          = yk62x86.delreg.Common

AddReg          = yk62x86.reg, yk62x86.common.params, yk62x86.YKVS_SL, yk62x86.GigFrSize.params, yk62x86.SingleLink.params, yk62x86.TxRxBuff.params, yk62x86.WoLStd.params, yk62x86.DefaultWfSOFF.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = yk62x86.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3


[SLYukFibGig_8000C774.ndi.NTx86.Services]
AddService      = yukonw7, 0x02, yukonw7.Service, common.EventLog


;-----------------------------------------------------------------------------
;
; General Driver Parameters
;
;-----------------------------------------------------------------------------
[yk62x86.common.params]
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, %IPChecksumOffloadIPv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, %TCPChecksumOffloadIPv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, %UDPChecksumOffloadIPv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR, Ndi\Params\NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,	Default,		0, ""
HKR, Ndi\Params\NetworkAddress,	Optional,		0, "1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, %InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, "enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, "1"

HKR, Ndi\Params\FixedIntMod,	ParamDesc,	0, %FixedIntMod%
HKR, Ndi\Params\FixedIntMod,	Type,		0, "int"
HKR, Ndi\Params\FixedIntMod,	Base,		0, "10"
HKR, Ndi\Params\FixedIntMod,	Min,			0, "1000"
HKR, Ndi\Params\FixedIntMod,	Max,			0, "30000"
HKR, Ndi\Params\FixedIntMod,	Step,		0, "1"
HKR, Ndi\Params\FixedIntMod,	Default,		0, "5000"

HKR, Ndi\Params\MessageLog,		ParamDesc,	0, %MessageLog%
HKR, Ndi\Params\MessageLog,		Type,		0, "enum"
HKR, Ndi\Params\MessageLog\enum,	"4",			0, %Non%
HKR, Ndi\Params\MessageLog\enum,	"3",			0, %Err%
HKR, Ndi\Params\MessageLog\enum,	"2",			0, %Wrn%
HKR, Ndi\Params\MessageLog\enum,	"1",			0, %Sta%
HKR, Ndi\Params\MessageLog\enum,	"0",			0, %All%
HKR, Ndi\Params\MessageLog,		Default,		0, "1"


;-----------------------------------------------------------------------------
;
; Driver parameters for IPv6 support
;
;-----------------------------------------------------------------------------
[yk62x86.IPv6.params]
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, %TCPChecksumOffloadIPv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, %UDPChecksumOffloadIPv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, "3"

[yk62x86.commonMsgLogOff.params]
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,		ParamDesc,	0, %TCPChecksumOffloadIPv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, %IPChecksumOffloadIPv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, %UDPChecksumOffloadIPv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, "3"


HKR, Ndi\Params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR, Ndi\Params\NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,	Default,		0, ""
HKR, Ndi\Params\NetworkAddress,	Optional,		0, "1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, %InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, "enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, "1"

HKR, Ndi\Params\FixedIntMod,	ParamDesc,	0, %FixedIntMod%
HKR, Ndi\Params\FixedIntMod,	Type,		0, "int"
HKR, Ndi\Params\FixedIntMod,	Base,		0, "10"
HKR, Ndi\Params\FixedIntMod,	Min,			0, "1000"
HKR, Ndi\Params\FixedIntMod,	Max,			0, "30000"
HKR, Ndi\Params\FixedIntMod,	Step,		0, "1"
HKR, Ndi\Params\FixedIntMod,	Default,		0, "5000"

HKR, Ndi\Params\MessageLog,		ParamDesc,	0, %MessageLog%
HKR, Ndi\Params\MessageLog,		Type,		0, "enum"
HKR, Ndi\Params\MessageLog\enum,	"4",			0, %Non%
HKR, Ndi\Params\MessageLog\enum,	"3",			0, %Err%
HKR, Ndi\Params\MessageLog\enum,	"2",			0, %Wrn%
HKR, Ndi\Params\MessageLog\enum,	"1",			0, %Sta%
HKR, Ndi\Params\MessageLog\enum,	"0",			0, %All%
HKR, Ndi\Params\MessageLog,		Default,		0, "4"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX buffers (V1 and V2)
;
;-----------------------------------------------------------------------------
[yk62x86.TxRxBuff.params]
HKR, Ndi\Params\*ReceiveBuffers,	ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,	Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,	Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,	Min,		0, "3"
HKR, Ndi\Params\*ReceiveBuffers,	Max,		0, "500"
HKR, Ndi\Params\*ReceiveBuffers,	Step,		0, "1"
HKR, Ndi\Params\*ReceiveBuffers,	Default,	0, "50"

HKR, Ndi\Params\*TransmitBuffers,ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,Min,		0, "4"
HKR, Ndi\Params\*TransmitBuffers,Max,		0, "200"
HKR, Ndi\Params\*TransmitBuffers,Step,		0, "1"
HKR, Ndi\Params\*TransmitBuffers,Default,	0, "50"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX LE (Y2)
;
;-----------------------------------------------------------------------------
[yk62x86.TxRxLE.params]
HKR, Ndi\Params\*ReceiveBuffers,	ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,	Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,	Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,	Min,		0, "256"
HKR, Ndi\Params\*ReceiveBuffers,	Max,		0, "512"
HKR, Ndi\Params\*ReceiveBuffers,	Step,		0, "256"
HKR, Ndi\Params\*ReceiveBuffers,	Default,	0, "256"

HKR, Ndi\Params\*TransmitBuffers,	ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,	Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,	Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,	Min,		0, "256"
HKR, Ndi\Params\*TransmitBuffers,	Max,		0, "512"
HKR, Ndi\Params\*TransmitBuffers,	Step,		0, "256"
HKR, Ndi\Params\*TransmitBuffers,	Default,	0, "256"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100/1000 chip)
;
;-----------------------------------------------------------------------------
[yk62x86.GigFrSize.params]
HKR, Ndi\params\*JumboPacket,	ParamDesc,	0, %JumboPacket%
HKR, Ndi\params\*JumboPacket,	Type,		0, "enum"
HKR, Ndi\params\*JumboPacket\enum,	"0",	0, "%Bytes1514%"
HKR, Ndi\params\*JumboPacket\enum,	"1",	0, "%Bytes4088%"
HKR, Ndi\params\*JumboPacket\enum,	"2",	0, "%Bytes9014%"
HKR, Ndi\params\*JumboPacket,	Default,	0, "0"
HKR,, *JumboPacket,, "0"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100 chip)
;
;-----------------------------------------------------------------------------
[yk62x86.FastFrSize.params]
HKR,, *JumboPacket,, "0"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for battery powered Adapters
;
;----------------------------------------------------------------------------
[yk62x86.BatMax.params]
HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatterySpeedSettings%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",		0, %SmartSpeed%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",		0, %MaxSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Default,	0, "4"

HKR, Ndi\Params\BatteryLinkDetectionMode,	ParamDesc,	0, %BatteryLinkDetectionMode%
HKR, Ndi\Params\BatteryLinkDetectionMode,	Type,		0, "enum"
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"0",		0, %NoPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"1",		0, %MaxPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"4",		0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode,	Default,	0, "4"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for smart battery powered Adapters
;
;----------------------------------------------------------------------------
[yk62x86.BatSmartDeep.params]
HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatterySpeedSettings%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",		0, %SmartSpeed%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",		0, %MaxSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Default,	0, "4"

HKR, Ndi\Params\BatteryLinkDetectionMode,	ParamDesc,	0, %SmartBatteryPowerSaving%
HKR, Ndi\Params\BatteryLinkDetectionMode,	Type,		0, "enum"
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"0",		0, %NoPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"4",		0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"5",		0, %DeepEnergySaving%
HKR, Ndi\Params\BatteryLinkDetectionMode,	Default,	0, "5"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for reduced battery powered Adapters
;
;-----------------------------------------------------------------------------
[yk62x86.BatMaxRed.params]
HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatterySpeedSettings%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",		0, %SmartSpeed%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",		0, %MaxSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Default,	0, "4"

HKR, Ndi\Params\BatteryLinkDetectionMode,		ParamDesc,	0, %BatteryLinkDetectionMode%
HKR, Ndi\Params\BatteryLinkDetectionMode,		Type,		0, "enum"
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"0",		0, %NoPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"4",		0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode,		Default,	0, "4"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for battery powered Adapters
;
;-----------------------------------------------------------------------------
[yk62x86.BatSmart.params]
HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatterySpeedSettings%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",		0, %SmartSpeed%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",		0, %MaxSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Default,	0, "3"

HKR, Ndi\Params\BatteryLinkDetectionMode,		ParamDesc,	0, %BatteryLinkDetectionMode%
HKR, Ndi\Params\BatteryLinkDetectionMode,		Type,		0, "enum"
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"0",		0, %NoPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"1",		0, %MaxPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,	"4",		0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryLinkDetectionMode,		Default,	0, "1"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan
;
;-----------------------------------------------------------------------------
[yk62x86.WoLStd.params]
HKR, Ndi\Params\WakeUpModeCap,		ParamDesc,	0, %WakeUpModeCap%
HKR, Ndi\Params\WakeUpModeCap,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap\enum,	"28",		0, %LinkChange%
HKR, Ndi\Params\WakeUpModeCap,		Default,	0, "27"

[yk62x86.DefaultWfSOFF.params]
HKR, Ndi\Params\WakeFromShutdown,		ParamDesc,	0, %WakeFromShutdown%
HKR, Ndi\Params\WakeFromShutdown,		Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",		0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",		0, %Off%
HKR, Ndi\Params\WakeFromShutdown,		Default,	0, "0"
HKR,, WakeFromShutdownMode,, "17"


[yk62x86.DefaultWfSON.params]
HKR, Ndi\Params\WakeFromShutdown,		ParamDesc,	0, %WakeFromShutdown%
HKR, Ndi\Params\WakeFromShutdown,		Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",		0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",		0, %Off%
HKR, Ndi\Params\WakeFromShutdown,		Default,	0, "1"
HKR,, WakeFromShutdownMode,, "17"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan variant 1
;
;-----------------------------------------------------------------------------
[yk62x86.WoLWfSForcedCombine.params]
HKR, Ndi\Params\WakeUpModeCap,		ParamDesc,	0, %WakeUpModeCap%
HKR, Ndi\Params\WakeUpModeCap,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap\enum,	"28",		0, %LinkChange%
HKR, Ndi\Params\WakeUpModeCap,		Default,	0, "27"

HKR,, WakeFromShutdown,, "1"
HKR,, WakeFromShutdownMode,, "17"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan variant 2
;
;-----------------------------------------------------------------------------
[yk62x86.WoLNoLnkCh.params]
HKR, Ndi\Params\WakeUpModeCap,		ParamDesc,	0, %WakeUpModeCap%
HKR, Ndi\Params\WakeUpModeCap,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap,		Default,	0, "27"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan variant 3
;
;-----------------------------------------------------------------------------
[yk62x86.WoLMagicPkt.params]
HKR, Ndi\Params\WakeUpModeCap,		ParamDesc,	0, %WakeUpModeCap%
HKR, Ndi\Params\WakeUpModeCap,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap,		Default,	0, "25"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan variant 4
;
;-----------------------------------------------------------------------------
[yk62x86.WoLMagicPktOnly.params]
HKR, Ndi\Params\WakeUpModeCap,		ParamDesc,	0, %WakeUpModeCap%
HKR, Ndi\Params\WakeUpModeCap,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap,		Default,	0, "25"

HKR,, WakeFromShutdownMode,, "17"

;-----------------------------------------------------------------------------
;
; Forced WoL defaults
;
;-----------------------------------------------------------------------------
[yk62x86.WoLMagicPacketDefault.params]
HKR,, WakeUpModeCap,, "25"

;-----------------------------------------------------------------------------
;
; Force WfS defaults
;
;-----------------------------------------------------------------------------


[yk62x86.WfSOFF.params]
HKR,, WakeFromShutdown,, "0"
HKR,, WakeFromShutdownMode,, "17"

[yk62x86.WfSON.params]
HKR,, WakeFromShutdown,, "1"
HKR,, WakeFromShutdownMode,, "17"

[yk62x86.WfSS5MagicPacket.params]
HKR,, WakeFromShutdown,, "1"
HKR,, WakeFromShutdownMode,, "17"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters
;
;-----------------------------------------------------------------------------
[yk62x86.WoLW10.params]
HKR,, WakeUpSpeed,, "2"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for Energy Star
;
;-----------------------------------------------------------------------------
[yk62x86.EnergyStarOn.params]
HKR, Ndi\Params\WakeUpSpeed,			ParamDesc,	0, %WakeUpSpeed%
HKR, Ndi\Params\WakeUpSpeed,			Type,		0, "enum"
HKR, Ndi\Params\WakeUpSpeed\enum,	"2",		0, %Enabled%
HKR, Ndi\Params\WakeUpSpeed\enum,	"3",		0, %Disabled%
HKR, Ndi\Params\WakeUpSpeed,			Default,	0, "2"


[yk62x86.EnergyStarOff.params]
HKR, Ndi\Params\WakeUpSpeed,			ParamDesc,	0, %WakeUpSpeed%
HKR, Ndi\Params\WakeUpSpeed,			Type,		0, "enum"
HKR, Ndi\Params\WakeUpSpeed\enum,	"2",		0, %Enabled%
HKR, Ndi\Params\WakeUpSpeed\enum,	"3",		0, %Disabled%
HKR, Ndi\Params\WakeUpSpeed,			Default,	0, "3"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters HwFeaDev
;
;-----------------------------------------------------------------------------

[yk62x86.HwFeaDev_1.params]
HKR,, HwFeaOnMask,,	"67108864"


[yk62x86.HwFeaDev_10.params]
HKR,, HwFeaOnMask,,	"36864"


[yk62x86.HwFeaDev_11.params]
HKR,, HwFeaOnMask,,	"201457664"


[yk62x86.HwFeaDev_2.params]
HKR,, HwFeaOnMask,,	"16777216"


[yk62x86.HwFeaDev_3.params]
HKR,, HwFeaOnMask,,	"201326592"


[yk62x86.HwFeaDev_4.params]
HKR,, HwFeaOnMask,,	"134348800"


[yk62x86.HwFeaDev_5.params]
HKR,, HwFeaOnMask,,	"8388608"


[yk62x86.HwFeaDev_6.params]
HKR,, HwFeaOnMask,,	"134217728"


[yk62x86.HwFeaDev_7.params]
HKR,, HwFeaOnMask,,	"32768"


[yk62x86.HwFeaDev_8.params]
HKR,, HwFeaOnMask,,	"134365184"


[yk62x86.HwFeaDev_9.params]
HKR,, HwFeaOnMask,,	"201474048"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for forced Batterymode defaults.
;
;-----------------------------------------------------------------------------
[yk62x86.SmartBatDefaults.params]
HKR,, BatterySpeedSettings,, "3"
HKR,, BatteryLinkDetectionMode,, "1"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for forced Batterymode defaults.
;
;-----------------------------------------------------------------------------
[yk62x86.FullBatDefaults.params]
HKR,, BatterySpeedSettings,, "4"
HKR,, BatteryLinkDetectionMode,, "1"

[yk62x86.BatMaxDefaults.params]
HKR,, BatterySpeedSettings,, "4"
HKR,, BatteryLinkDetectionMode,, "4"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TCP segmentation
;
;-----------------------------------------------------------------------------
[yk62x86.TcpSegm.params]
HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, %LsoV1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, "1"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TCP segmentation with default value set to Off.
;
;-----------------------------------------------------------------------------
[yk62x86.TcpSegmLSOff.params]

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, %LsoV1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, "0"

HKR,, *LsoV1IPv4,,  "0"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for large send
;
;-----------------------------------------------------------------------------
[yk62x86.LsoV2.params]
HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0, %LsoV2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,	"1",	0,	%Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,	"0",	0,	%Disabled%
HKR, Ndi\Params\*LsoV2IPv4,	Default,	0,	"1"

HKR,, *LsoV2IPv4,,  "1"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0, %LsoV2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,	"1",	0,	%Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,	"0",	0,	%Disabled%
HKR, Ndi\Params\*LsoV2IPv6,	Default,	0,	"1"

HKR,, *LsoV2IPv6,,  "1"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for RSS
;
;-----------------------------------------------------------------------------
[yk62x86.RSS.params]
HKR, Ndi\Params\*RSS,			ParamDesc,	0, %RSS%
HKR, Ndi\Params\*RSS,			Type,		0, "enum"
HKR, Ndi\Params\*RSS\enum,	"1",	0,	%Enabled%
HKR, Ndi\Params\*RSS\enum,	"0",	0,	%Disabled%
HKR, Ndi\Params\*RSS,	Default,	0,	"0"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Single Link Adapters
;
;-----------------------------------------------------------------------------
[yk62x86.SingleLink.params]

HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowControl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "3"
HKR,, *FlowControl,, "3"

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Single Link Adapters (FlowControl OFF)
;
;-----------------------------------------------------------------------------
[yk62x86.SingleLinkFCOff.params]
HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowControl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "0"
HKR,, *FlowControl,, "0"

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"

;-----------------------------------------------------------------------------
;
; Additional driver parameter to set the port speed and capabilities
;
;-----------------------------------------------------------------------------
[yk62x86.SLSpeedDuplex.params]
HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "0"
HKR,Ndi\Params\*SpeedDuplex\enum, "0",        0, %Autosense%
HKR,Ndi\Params\*SpeedDuplex\enum, "1",        0, %10MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "2",        0, %10MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%


[yk62x86.SLSpeedDuplexGig.params]
HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "0"
HKR,Ndi\Params\*SpeedDuplex\enum, "0",        0, %Autosense%
HKR,Ndi\Params\*SpeedDuplex\enum, "1",        0, %10MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "2",        0, %10MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "5",        0, %1000MFD%

[yk62x86.SLSpeedDuplex_100M_only.params]
HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "4"
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%



;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Dual Link Adapters
;
;-----------------------------------------------------------------------------
[yk62x86.DualLink.params]
HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowControl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "3"

HKR, Ndi\Params\RlmtMode,		ParamDesc,	0, %RlmtMode%
HKR, Ndi\Params\RlmtMode,		Type,		0, "enum"
HKR, Ndi\Params\RlmtMode\enum,	"1",		0, %Link%
HKR, Ndi\Params\RlmtMode\enum,	"3",		0, %OtherPort%
HKR, Ndi\Params\RlmtMode\enum,	"7",		0, %Segment%
HKR, Ndi\Params\RlmtMode,		Default,	0, "1"

HKR, Ndi\Params\PreferredPort,		ParamDesc,	0, %PreferredPort%
HKR, Ndi\Params\PreferredPort,		Type,		0, "enum"
HKR, Ndi\Params\PreferredPort\enum,	"1",		0, %A%
HKR, Ndi\Params\PreferredPort\enum,	"2",		0, %B%
HKR, Ndi\Params\PreferredPort,		Default,	0, "1"

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"
HKR,, RlmtChgBCPrio,, 		 "0"



[yk62x86.DLSpeedDuplexGig.params]

HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "0"
HKR,Ndi\Params\*SpeedDuplex\enum, "0",        0, %Autosense%
HKR,Ndi\Params\*SpeedDuplex\enum, "1",        0, %10MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "2",        0, %10MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "5",        0, %1000MFD%


;-----------------------------------------------------------------------------
;
; Power Management
;
;-----------------------------------------------------------------------------

[yk62x86.SmartPowMgmt.params]

;Key used by notify object
HKR,, SmartPowMgmtProfile,, "3"
HKR,, SmartPowMgmtLinkDetection,, "1"


[yk62x86.MonitorSpeedStep.params]

;Key used by notify object
HKR,, MonitorSpeedStep,, "1"


;-----------------------------------------------------------------------------
;
; Property Page 
;
;-----------------------------------------------------------------------------

[yk62x86.PropPage_PMChkBox_x00.params]
;Allow computer to turn off device (case 1)
HKR,, PnPCapabilities,0x00010001, 0x10

[yk62x86.PropPage_PMChkBox_xx0.params]
;Allow device to bring computer out of standby (case 2)
HKR,, PnPCapabilities,0x00010001, 0x0

[yk62x86.PropPage_PMChkBox_xxx.params]
;allow device to wake up PC via MagicPacket (case 3)
HKR,, PnPCapabilities,0x00010001, 0x100
;-----------------------------------------------------------------------------
;
; General Registry Entries
;
;-----------------------------------------------------------------------------
[yk62x86.reg]

HKR, Ndi\Interfaces, UpperRange,, "ndis5"

HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "yukonw7"

;-----------------------------------------------------------------------------
;
; Special Registry Entrries
;
;-----------------------------------------------------------------------------
[yk62x86.YKVS_SL]

;Key used by notify object
HKR,, YKVS,, "762751"
;-----------------------------------------------------------------------------
;
; Special Registry Entries
;
;-----------------------------------------------------------------------------
[yk62x86.YKVS_DL]

;Key used by notify object
HKR,, YKVS,, "762752"


;-----------------------------------------------------------------------------
;
; This section contain the keys which will be deleted. These are old keys
; which are not any more supported in newest INF.
;
;-----------------------------------------------------------------------------
[yk62x86.delreg.Common]
HKR, Ndi\Params\MaxFrameSize
HKR, Ndi\Params\HwChecksum
HKR, Ndi\Params\Moderate
HKR, Ndi\Params\MaxReceives
HKR, Ndi\Params\MaxTransmits
HKR, Ndi\Params\BatteryModeLinkDetection
HKR, Ndi\Params\TcpLargeSend
HKR, Ndi\Params\WakeUpModeCap_A
HKR, Ndi\Params\WakeUpModeCap_B
HKR, Ndi\Params\DuplexCapabilities_A
HKR, Ndi\Params\DuplexCapabilities_B
HKR, Ndi\Params\FlowControl_A
HKR, Ndi\Params\FlowControl_B
HKR, Ndi\Params\AutoNegotiation_A
HKR, Ndi\Params\AutoNegotiation_B
HKR, Ndi\Params\Role_A
HKR, Ndi\Params\Role_B
HKR, Ndi\Params\Speed_A
HKR, Ndi\Params\Speed_B
HKR, Ndi\Params\TagHeaderSupport_A
HKR, Ndi\Params\TagHeaderSupport_B
HKR, Ndi\Params\FlowControl_A
HKR, Ndi\Params\FlowControl_B
HKR, Ndi\Params\ConnectionType_A
HKR, Ndi\Params\ConnectionType_B
HKR, Ndi\Params\*NetworkAddress
HKR, Ndi\Params\*JumboPacket\enum,1514
HKR, Ndi\Params\*JumboPacket\enum,4088
HKR, Ndi\Params\*JumboPacket\enum,9014
HKR, Ndi\Params\*PriorityVLANTag
HKR,, HwChecksum
HKR,, Moderate
HKR,, MaxReceives
HKR,, MaxTransmits
HKR,, BatteryModeLinkDetection
HKR,, TcpLargeSend
HKR,, WakeUpModeCap_A
HKR,, WakeUpModeCap_B
HKR,, DuplexCapabilities_A
HKR,, DuplexCapabilities_B
HKR,, AutoNegotiation_A
HKR,, AutoNegotiation_B
HKR,, Role_A
HKR,, Role_B
HKR,, Speed_A
HKR,, Speed_B
HKR,, TagHeaderSupport_A
HKR,, TagHeaderSupport_B
HKR,, FlowControl_A
HKR,, FlowControl_B
HKR,, ConnectionType_A
HKR,, ConnectionType_B
HKR,, *NetworkAddress
HKR,, *PriorityVLANTag



;-----------------------------------------------------------------------------
;
; This section contain the keys which will be deleted. These are old keys
; which are not any more supported in newest INF.
;
;-----------------------------------------------------------------------------
[yk62x86.delreg.WfSSL]

; remove the "WakeFromShutdown" key.
HKR, Ndi\Params\WakeFromShutdown
HKR,, WakeFromShutdown

[yk62x86.delreg.WfSSLParam]

; remove the "WakeFromShutdown" key.
HKR, Ndi\Params\WakeFromShutdown


[yk62x86.delreg.PatternMatch]
HKR, Ndi\Params\WakeUpModeCap\enum,26

[yk62x86.delreg.MagPackPattMatch]
HKR, Ndi\Params\WakeUpModeCap\enum,27

[yk62x86.delreg.LinkChange]
HKR, Ndi\Params\WakeUpModeCap\enum,28


[yk62x86.delreg.WoLAll]
HKR, Ndi\Params\WakeUpModeCap
HKR, Ndi\Params\WakeFromShutdown
HKR,, WakeUpModeCap
HKR,, WakeFromShutdown


[yk62x86.delreg.TcpLargeSend]
HKR, Ndi\Params\TcpLargeSend
HKR,, TcpLargeSend



[yk62x86.delreg.BatParams]
HKR, Ndi\Params\BatterySpeedSettings
HKR,, BatterySpeedSettings
HKR, Ndi\Params\BatteryLinkDetectionMode
HKR,, BatteryLinkDetectionMode

[yk62x86.delreg.SmartPowMgmt]
HKR,, SmartPowMgmtProfile
HKR,, SmartPowMgmtLinkDetection
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,5


[yk62x86.delreg.JumboPacket]
HKR, Ndi\params\*JumboPacket
HKR,, *JumboPacket

[yk62x86.delreg.MaxPwrSaveMode]
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,1

[yk62x86.delreg.SpeedDuplexNot100]
HKR, Ndi\Params\BatteryLinkDetectionMode\enum,1
HKR, Ndi\Params\*SpeedDuplex\enum, 0
HKR, Ndi\Params\*SpeedDuplex\enum, 1
HKR, Ndi\Params\*SpeedDuplex\enum, 2
HKR, Ndi\Params\*SpeedDuplex\enum, 5



;-----------------------------------------------------------------------------
;
; Service
;
;-----------------------------------------------------------------------------
[yukonw7.Service]
DisplayName	= %yk62x86.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\yk62x86.sys
LoadOrderGroup = NDIS

;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.EventLog]
AddReg = common.AddEventLog.reg

;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\yk62x86.sys"
HKR,, TypesSupported,	0x00010001, 7


;-----------------------------------------------------------------------------
;
; Source Files
;
;-----------------------------------------------------------------------------
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
yk62x86.sys	= 1,,

[yk62x86.CopyFiles]
yk62x86.sys,,,2


;-----------------------------------------------------------------------------
;
; Destination Directories
;
;-----------------------------------------------------------------------------
[DestinationDirs]

DefaultDestDir = 12
yk62x86.CopyFiles=	12

;-----------------------------------------------------------------------------
;
; Localizable Strings
;
;-----------------------------------------------------------------------------
[Strings]

Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Jumbo Packet"
ReceiveBuffers = "Receive Buffers"
TransmitBuffers = "Transmit Buffers"
IPChecksumOffloadIPv4 = "IPv4 Checksum Offload"
TCPChecksumOffloadIPv4 = "TCP Checksum Offload (IPv4)"
TCPChecksumOffloadIPv6 = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadIPv4 = "UDP Checksum Offload (IPv4)"
UDPChecksumOffloadIPv6 = "UDP Checksum Offload (IPv6)"
LsoV1IPv4 = "Large Send Offload (IPv4)"
LsoV2IPv4 = "Large Send Offload v2 (IPv4)"
LsoV2IPv6 = "Large Send Offload v2 (IPv6)"
RSS = "Receive-Side Scaling"
TXEna = "Tx Enabled"
RXEna = "Rx Enabled"
TXRXEna = "Tx & Rx Enabled"
NetworkAddress   = "Network Address"
WakeUpModeCap   = "Wake-Up Capabilities"
InterruptModeration = "Interrupt Moderation"
FixedIntMod = "Max IRQ per Sec"
MessageLog = "Log Status Messages"
RlmtMode  = "RLMT Mode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
PreferredPort = "Preferred Port"
On = "On"
Off = "Off"
Enabled = "Enabled"
Disabled = "Disabled"
Non = "None"
Err = "Errors"
Wrn = "Warnings"
Sta = "Status Messages"
All = "All Messages"
A = "A"
B = "B"
Autosense = "Auto-Negotiation"
10MHD = "10 Mbps Half Duplex"
10MFD = "10 Mbps Full Duplex"
100MHD = "100 Mbps Half Duplex"
100MFD = "100 Mbps Full Duplex"
1000MFD = "1000 Mbps Full Duplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Link Change"
SpeedDuplex = "Speed & Duplex"
FlowControl = "Flow Control"
WakeFromShutdown = "Wake From Shutdown"
BatterySpeedSettings = "Battery Speed Settings"
SmartSpeed = "Smart Speed Down"
MaxSpeed = "Full Speed"
BatteryLinkDetectionMode = "Battery Mode Link Detection"
NoPwrSave = "No Energy Saving"
MaxPwrSave = "Maximum Energy Saving"
EnDetPwrSave = "EnergyDetect+™"
SmartBatteryPowerSaving = "Smart Battery Power Saving"
DeepEnergySaving = "Deep Energy Saving"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
WakeUpSpeed = "Energy Star"
;-----------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"

AT-2803.DeviceDesc = "Allied Telesis AT-2814FX"
AT-2804.DeviceDesc = "Allied Telesis AT-2874xx"
AT-2916.DeviceDesc = "Allied Telesis AT-2916T"
AT-2973.DeviceDesc = "Allied Telesis AT-2971SX v1 Gigabit Adapter"
AT-2973_1.DeviceDesc = "Allied Telesis AT-2971SX v2 Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesis AT-2971T v1 Gigabit Adapter"
AT-2974_1.DeviceDesc = "Allied Telesis AT-2971T v2 Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesis AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E21M.DeviceDesc = "SysKonnect SK-9E21M 10/100/1000Base-T Adapter for DASH 1.0"
SKYukon2-9E21M_1.DeviceDesc = "SysKonnect SK-9E21M 10/100/1000Base-T Adapter for DASH 1.1"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1032.DeviceDesc = "Linksys EG1032 v2 Instant Gigabit Network Adapter"
Yukon-1064.DeviceDesc = "Linksys EG1064 v2 Instant Gigabit Network Adapter"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4354.DeviceDesc = "Marvell Yukon 88E8040 PCI-E Fast Ethernet Controller"
Yukon-4355.DeviceDesc = "Marvell Yukon 88E8040T PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4357.DeviceDesc = "Marvell Yukon 88E8042 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4365.DeviceDesc = "Marvell Yukon 88E8070 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-436A.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-436B.DeviceDesc = "Marvell Yukon 88E8071 PCI-E Gigabit Ethernet Controller"
Yukon-436C.DeviceDesc = "Marvell Yukon 88E8072 PCI-E Gigabit Ethernet Controller"
Yukon-4370.DeviceDesc = "Marvell Yukon 88E8075 PCI-E Gigabit Ethernet Controller"
Yukon-4380.DeviceDesc = "Marvell Yukon 88E8057 PCI-E Gigabit Ethernet Controller"
Yukon-4381.DeviceDesc = "Marvell Yukon 88E8059 PCI-E Gigabit Ethernet Controller"
Yukon-4382.DeviceDesc = "Marvell Yukon 88E8079 PCI-E Gigabit Ethernet Controller"
Yukon-Generic.DeviceDesc = "Generic Marvell Yukon 88E8001/8003/8010 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8048 PCI-E Fast Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Marvell Yukon 88E8057 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88E8058 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_20.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_21.DeviceDesc = "Generic Marvell Yukon 88E8070 based Ethernet Controller"
Yukon-Generic_22.DeviceDesc = "Generic Marvell Yukon 88E8071 based Ethernet Controller"
Yukon-Generic_23.DeviceDesc = "Generic Marvell Yukon 88E8072 based Ethernet Controller"
Yukon-Generic_24.DeviceDesc = "Generic Marvell Yukon 88E8075 based Ethernet Controller"
Yukon-Generic_25.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_26.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_27.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_28.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_29.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_30.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Marvell Yukon 88E8040 Family PCI-E Fast Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8040T PCI-E Fast Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8042 PCI-E Fast Ethernet Controller"
yk62x86.DriverDesc = "NDIS6.2 Miniport Driver for Marvell Yukon Ethernet Controller"


;-----------------------------------------------------------------------------

; Chinese (PRC)
[Strings.0804]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "巨型包"
ReceiveBuffers = "接收缓冲区"
TransmitBuffers = "传送缓冲区"
IPChecksumOffloadIPv4 = "卸载 IPv4 校验和"
TCPChecksumOffloadIPv4 = "卸载 TCP 校验和 (IPv4)"
TCPChecksumOffloadIPv6 = "卸载 TCP 校验和 (IPv6)"
UDPChecksumOffloadIPv4 = "卸载 UDP 校验和 (IPv4)"
UDPChecksumOffloadIPv6 = "卸载 UDP 校验和 (IPv6)"
LsoV1IPv4 = "大量传送负载 (IPv4)"
LsoV2IPv4 = "大量传送负载 v2 (IPv4)"
LsoV2IPv6 = "大量传送负载 v2 (IPv6)"
RSS = "接收端调整"
TXEna = "启用 Tx"
RXEna = "启用 Rx"
TXRXEna = "启用Tx 和 Rx"
NetworkAddress   = "网络地址"
WakeUpModeCap   = "唤醒功能"
InterruptModeration = "中断模式"
FixedIntMod = "最大 IRQ数量"
MessageLog = "日志状态信息"
RlmtMode  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
PreferredPort    = "首选端口"
On = "开"
Off = "关"
Enabled = "启用"
Disabled = "禁用"
Non = "无"
Err = "错误"
Wrn = "警告"
Sta = "状态信息"
All = "所有信息"
A = "A"
B = "B"
Autosense = "自动感应"
10MHD = "10Mbps 半双工"
10MFD = "10Mbps 全双工"
100MHD = "100Mbps 半双工"
100MFD = "100Mbps 全双工"
1000MFD = "1000Mbps 全双工"
MagicPacket = "Magic Packet唤醒模式"
PatternMatch = "Pattern Match唤醒模式"
MagPackPattMatch = "MP 和 PM 唤醒模式"
LinkChange = "Link Change唤醒模式"
SpeedDuplex = "速度和双工"
FlowControl = "流控制"
WakeFromShutdown = "从关闭中唤醒"
BatterySpeedSettings = "电池消耗速度设置"
SmartSpeed = "较慢电池消耗速度"
MaxSpeed = "最快电池消耗速度"
BatteryLinkDetectionMode = "电池模式连接检测"
NoPwrSave = "无电量节省"
MaxPwrSave = "最大电量节省"
EnDetPwrSave = "很大电量节省+ (EnergyDetect+™)"
SmartBatteryPowerSaving = "Smart Battery Power Saving"
DeepEnergySaving = "Deep Energy Saving"
Bytes1514 = "1514 个字节"
Bytes4088 = "4088 个字节"
Bytes9014 = "9014 个字节"
WakeUpSpeed = "能量之星 (Energy Star)"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


AT-2803.DeviceDesc = "Allied Telesis AT-2814FX"
AT-2804.DeviceDesc = "Allied Telesis AT-2874xx"
AT-2916.DeviceDesc = "Allied Telesis AT-2916T"
AT-2973.DeviceDesc = "Allied Telesis AT-2971SX v1 Gigabit Adapter"
AT-2973_1.DeviceDesc = "Allied Telesis AT-2971SX v2 Gigabit Adapter"
AT-2974.DeviceDesc = "Allied Telesis AT-2971T v1 Gigabit Adapter"
AT-2974_1.DeviceDesc = "Allied Telesis AT-2971T v2 Gigabit Adapter"
AT-2978.DeviceDesc = "Allied Telesis AT-2971LX Gigabit Adapter"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SKYukon2-2220.DeviceDesc = "TPMC-GBE-CO"
SKYukon2-8220.DeviceDesc = "TPMC-GBE-FI"
SKYukon2-9C21.DeviceDesc = "SysKonnect SK-9C21 10/100/1000Base-T Adapter, ExpressCard"
SKYukon2-9E21.DeviceDesc = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express, Copper RJ-45"
SKYukon2-9E21D.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express, Copper RJ-45"
SKYukon2-9E21M.DeviceDesc = "SysKonnect SK-9E21M 10/100/1000Base-T Adapter for DASH 1.0"
SKYukon2-9E21M_1.DeviceDesc = "SysKonnect SK-9E21M 10/100/1000Base-T Adapter for DASH 1.1"
SKYukon2-9E22.DeviceDesc = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express, 2 Copper RJ-45"
SKYukon2-9E81.DeviceDesc = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express, Fiber SX/LC"
SKYukon2-9E82.DeviceDesc = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express, 2 Fiber SX/LC"
SKYukon2-9E91.DeviceDesc = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express, Fiber LX/LC"
SKYukon2-9E92.DeviceDesc = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express, 2 Fiber LX/LC"
SKYukon2-9I22.DeviceDesc = "SysKonnect SK-9I22 10/100/1000 Base-T Dual Port Express Module"
SKYukon2-9P22.DeviceDesc = "SysKonnect SK-9P22 10/100/1000 Base-T Dual Port PMC card"
SKYukon2-9P82.DeviceDesc = "SysKonnect SK-9P82 1000 Base-SX Dual Port PMC card"
SKYukon2-9S21.DeviceDesc = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45"
SKYukon2-9S22.DeviceDesc = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X, 2 Copper RJ-45"
SKYukon2-9S81.DeviceDesc = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X, Fiber SX/LC"
SKYukon2-9S82.DeviceDesc = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X, 2 Fiber SX/LC"
SKYukon2-9S91.DeviceDesc = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X, Fiber LX/LC"
SKYukon2-9S92.DeviceDesc = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X, 2 Fiber LX/LC"
Yukon-1032.DeviceDesc = "Linksys EG1032 v2 Instant Gigabit Network Adapter"
Yukon-1064.DeviceDesc = "Linksys EG1064 v2 Instant Gigabit Network Adapter"
Yukon-1700.DeviceDesc = "3Com 3C2000-T Gigabit Adapter"
Yukon-1700_1.DeviceDesc = "3Com 3C940 Gigabit LOM Ethernet Adapter"
Yukon-4320.DeviceDesc = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon-4340.DeviceDesc = "Marvell Yukon 88E8021 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4341.DeviceDesc = "Marvell Yukon 88E8022 PCI-X IPMI Gigabit Ethernet Controller"
Yukon-4342.DeviceDesc = "Marvell Yukon 88E8061 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4343.DeviceDesc = "Marvell Yukon 88E8062 PCI-E IPMI Gigabit Ethernet Controller"
Yukon-4350.DeviceDesc = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon-4351.DeviceDesc = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon-4352.DeviceDesc = "Marvell Yukon 88E8038 PCI-E Fast Ethernet Controller"
Yukon-4353.DeviceDesc = "Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-4354.DeviceDesc = "Marvell Yukon 88E8040 PCI-E Fast Ethernet Controller"
Yukon-4355.DeviceDesc = "Marvell Yukon 88E8040T PCI-E Fast Ethernet Controller"
Yukon-4356.DeviceDesc = "Marvell Yukon 88EC033 PCI-E Fast Ethernet Controller"
Yukon-4357.DeviceDesc = "Marvell Yukon 88E8042 PCI-E Fast Ethernet Controller"
Yukon-4360.DeviceDesc = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4361.DeviceDesc = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon-4362.DeviceDesc = "Gigabit ExpressCard Adapter"
Yukon-4362_1.DeviceDesc = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon-4362_2.DeviceDesc = "PLANEX GEX-1000T ExpressCard Gigabit LAN Adapter"
Yukon-4363.DeviceDesc = "Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-4364.DeviceDesc = "Marvell Yukon 88E8056 PCI-E Gigabit Ethernet Controller"
Yukon-4365.DeviceDesc = "Marvell Yukon 88E8070 PCI-E Gigabit Ethernet Controller"
Yukon-4366.DeviceDesc = "Marvell Yukon 88EC036 PCI-E Gigabit Ethernet Controller"
Yukon-4369.DeviceDesc = "Marvell Yukon 88EC042 PCI-E Gigabit Ethernet Controller"
Yukon-436A.DeviceDesc = "Marvell Yukon 88E8058 PCI-E Gigabit Ethernet Controller"
Yukon-436B.DeviceDesc = "Marvell Yukon 88E8071 PCI-E Gigabit Ethernet Controller"
Yukon-436C.DeviceDesc = "Marvell Yukon 88E8072 PCI-E Gigabit Ethernet Controller"
Yukon-4370.DeviceDesc = "Marvell Yukon 88E8075 PCI-E Gigabit Ethernet Controller"
Yukon-4380.DeviceDesc = "Marvell Yukon 88E8057 PCI-E Gigabit Ethernet Controller"
Yukon-4381.DeviceDesc = "Marvell Yukon 88E8059 PCI-E Gigabit Ethernet Controller"
Yukon-4382.DeviceDesc = "Marvell Yukon 88E8079 PCI-E Gigabit Ethernet Controller"
Yukon-Generic.DeviceDesc = "Generic Marvell Yukon 88E8001/8003/8010 based Ethernet Controller"
Yukon-Generic_1.DeviceDesc = "Generic Marvell Yukon 88E8021 based Ethernet Controller"
Yukon-Generic_10.DeviceDesc = "Generic Marvell Yukon 88E8048 PCI-E Fast Ethernet Controller"
Yukon-Generic_11.DeviceDesc = "Generic Marvell Yukon 88E8050 based Ethernet Controller"
Yukon-Generic_12.DeviceDesc = "Generic Marvell Yukon 88E8052 based Ethernet Controller"
Yukon-Generic_13.DeviceDesc = "Generic Marvell Yukon 88E8053 based Ethernet Controller"
Yukon-Generic_14.DeviceDesc = "Generic Marvell Yukon 88E8055 PCI-E Gigabit Ethernet Controller"
Yukon-Generic_15.DeviceDesc = "Generic Marvell Yukon 88E8056 based Ethernet Controller"
Yukon-Generic_16.DeviceDesc = "Marvell Yukon 88E8057 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_17.DeviceDesc = "Generic Marvell Yukon 88E8058 based Ethernet Controller"
Yukon-Generic_18.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_19.DeviceDesc = "Generic Marvell Yukon 88E8061 based Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Generic Marvell Yukon 88E8022 based Ethernet Controller"
Yukon-Generic_20.DeviceDesc = "Generic Marvell Yukon 88E8062 based Ethernet Controller"
Yukon-Generic_21.DeviceDesc = "Generic Marvell Yukon 88E8070 based Ethernet Controller"
Yukon-Generic_22.DeviceDesc = "Generic Marvell Yukon 88E8071 based Ethernet Controller"
Yukon-Generic_23.DeviceDesc = "Generic Marvell Yukon 88E8072 based Ethernet Controller"
Yukon-Generic_24.DeviceDesc = "Generic Marvell Yukon 88E8075 based Ethernet Controller"
Yukon-Generic_25.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_26.DeviceDesc = "Generic Marvell Yukon 88EC032 based Ethernet Controller"
Yukon-Generic_27.DeviceDesc = "Generic Marvell Yukon 88EC033 based Ethernet Controller"
Yukon-Generic_28.DeviceDesc = "Generic Marvell Yukon 88EC034 based Ethernet Controller"
Yukon-Generic_29.DeviceDesc = "Generic Marvell Yukon 88EC036 PCI-E Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Generic Marvell Yukon 88E8035 based Ethernet Controller"
Yukon-Generic_30.DeviceDesc = "Generic Marvell Yukon 88EC042 based Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Generic Marvell Yukon 88E8036 based Ethernet Controller"
Yukon-Generic_5.DeviceDesc = "Generic Marvell Yukon 88E8038 based Ethernet Controller"
Yukon-Generic_6.DeviceDesc = "Generic Marvell Yukon 88E8039 PCI-E Fast Ethernet Controller"
Yukon-Generic_7.DeviceDesc = "Marvell Yukon 88E8040 Family PCI-E Fast Ethernet Controller"
Yukon-Generic_8.DeviceDesc = "Generic Marvell Yukon 88E8040T PCI-E Fast Ethernet Controller"
Yukon-Generic_9.DeviceDesc = "Generic Marvell Yukon 88E8042 PCI-E Fast Ethernet Controller"
yk62x86.DriverDesc = "NDIS6.2 Miniport Driver for Marvell Yukon Ethernet Controller"
