
       Оптимизированный драйвер INTEL Graphics 9.18.10.3293 для использования в PE_7x86, PE_8x86.

    Драйвер пригоден для установщика DevInst.exe или стандартного обновления устройств.

    Для стандартного обновления устройств распакуйте драйвер до уровня каталога с файлами.

--------------------------------------------------------------------------------------------------

      Драйвер INTEL Graphics 9.18.10.3293 Windows 7/8 (32 bit), каталог IG918103293_NT6x32.     

    DriverVer = 09/03/2013, 9.18.10.3293. Отключены OpenCL, OpenGL, ControlPanel. Product Support:

  Supports Intel(R) Iris(TM) graphics, Intel(R) Iris(TM) Pro graphics and Intel(R) HD graphics on: 

    4th Generation Intel(R) Core(TM) Processor Platform
    4th Generation Intel(R) Core(TM) Processor U Series based Platform
    3rd Generation Intel(R) Core(TM) Processor Platform
    3rd Generation Intel(R) Core(TM) Processor U Series based Platform
    3rd Generation Intel(R) Core(TM) Processor Y Series based Platform
    Intel(R) Pentium(R) Processor 2000/3000/G2000/G2100/G3000 Series 
    Intel(R) Celeron(R) Processor 900/1000/2000/G1000 Series

--------------------------------------------------------------------------------------------------

    ; 3rd Generation Intel® IvyBridge HD Graphics
    iIVBGD0       = "(PE) Intel(R) 3rd Generation IvyBridge HD Graphics 4000"
    iIVBGM0       = "(PE) Intel(R) 3rd Generation IvyBridge HD Graphics 4000"
    iIVBGD0SRV    = "(PE) Intel(R) 3rd Generation IvyBridge HD Graphics P4000"
    iIVBGD0GT1    = "(PE) Intel(R) 3rd Generation IvyBridge HD Graphics GT1"
    iIVBGM0GT1    = "(PE) Intel(R) 3rd Generation IvyBridge HD Graphics GT1"
    iIVBGD0SRVGT1 = "(PE) Intel(R) 3rd Generation IvyBridge HD / Server Graphics GT1"

    ; 4th Generation Intel® Haswell HD Graphics
    iHSWGT1D   	  = "(PE) Intel(R) 4th Generation Haswell HD Graphics"
    iHSWGT1M      = "(PE) Intel(R) 4th Generation Haswell HD Graphics"
    iHSWGT15D     = "(PE) Intel(R) 4th Generation Haswell HD Graphics 4400"
    iHSWGT2D      = "(PE) Intel(R) 4th Generation Haswell HD Graphics 4600"
    iHSWGT2M      = "(PE) Intel(R) 4th Generation Haswell HD Graphics 4600"
    ; HSW ULT
    iHSWGT1UT     = "(PE) Intel(R) 4th Generation Haswell Intel(R) HD Graphics"
    iHSWGT2UT     = "(PE) Intel(R) 4th Generation Haswell HD Graphics Family"
    iHSWGT3UT     = "(PE) Intel(R) 4th Generation Haswell HD Graphics 5000"
    iHSWGT3UT28W  = "(PE) Intel(R) 4th Generation Haswell Iris(TM) Graphics 5100"
    iHSWGT2UX     = "(PE) Intel(R) 4th Generation Haswell HD Graphics Family"
    iHSWGT1ULX	  = "(PE) Intel(R) 4th Generation Haswell HD Graphics"
    ; HSW CRW
    iHSWGT3CW     = "(PE) Intel(R) 4th Generation Haswell Iris(TM) Pro Graphics 5200"
    iHSWGT3CWDT   = "(PE) Intel(R) 4th Generation Haswell Iris(TM) Pro Graphics 5200"
    ; HSW SRVR
    iHSWSVGT1     = "(PE) Intel(R) 4th Generation Haswell HD Graphics"
    iHSWSVGT2  	  = "(PE) Intel(R) 4th Generation Haswell HD Graphics P4600/P4700"

       
--------------------------------------------------------------------------------------------------

      В случае установки драйвера  видеоадаптера  через диспетчер устройств,  необходимо выполнить

    детект PnP устройств или запустить утилиту типа Resolution Changer SX2 для того чтобы заменить

    пока еще работающий стандартный VGA драйвер  (иначе появляется ошибка при изменении параметров

    экрана).  При подключении  посредством  DevInst.exe автоматически  устанавливается оптимальное

    разрешение и частота регенерации для обнаруженного типа монитора.

==================================================================================================
 01-Oct-2013 nat27 http://forum.ru-board.com/topic.cgi?forum=62&topic=24098&start=71&limit=1&m=1#1
==================================================================================================
  